<page>030r</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f65.image</image>

<div>  
<id>p030r\_a1</id>  
<head><m>Lead</m></head>

<ab>The best, fattest &amp; softest is brought from <pl>Germany</pl> and is not in <fr>saulmon</fr>, but in <fr>lattes</fr>, of around an <ms><bp>arm</bp></ms> long &amp; three <ms><bp>fingers</bp></ms> wide. It is transported to <pl>Lyon</pl>, and from this, the leaf is made for small mirrors in <pl>Nuremberg</pl>.</ab>

</div>

<div>  
<id>p030r\_a2</id>  
<head><pro>Pewterer</pro></head>

<ab>They also make their <tl>molds</tl> out of <m>metal</m> which last longer &amp; mold more cleanly than <m><fr>grais</fr></m>, because the vessel comes out without fins &amp; smooth. But this is for the <pro>rich</pro> because a <tl>mold</tl> costs fifteen or sixteen <cn>frans</cn>. They are mainly made of <m>metal</m>, for basins &amp; ewers &amp; salt cellars &amp; similar things which are fashioned.</ab>

<ab>For pints, <tl>molds</tl> are made with <m>white clay</m> mixed with <m><al>horse</al> dung</m> &amp; <m>cloth waste</m> &amp; well beaten, because the pints, being deep half-circles, would not easily release from the <tl><m><fr>grais</fr></m> mould</tl>, unlike the <m>earth</m> ones, which are soft. One makes the <fr>noyau</fr> of the <tl>mold</tl> of the said pints in <fr>grais</fr>.</ab>

<ab>In <tl>metal molds</tl>, one makes vents and casts all at once, which is the cause that in the middle of the dish, no smoky black line which comes from the vapor &amp; smoke of the <m>metal</m> that is cast, which is the cause that in that spot, the work is lumpy &amp; very often pierced. However they repair it with <m>soldering</m> <del><fr>du n</fr></del>, as is said. This smoke is made right in the middle of the cast, &amp; in <tl> molds of <m><fr>grais</fr></m></tl>.</ab>

<ab>The vessel can be <tl>hammered</tl> <del><fr>mar</fr></del> to make it more vendable. But it will not last as long.</ab>

<ab>Depending on the size of their dishes &amp; plates, they have notches on the spoke of their <tl><m>iron</m> wheels</tl>. And when they want to apply</ab>

<cont/>

</div>