<page>043v</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f92.image</image>

<div>

<id>p043v\_1</id>

<head><m>Varied and transmuted wine</m></head>

<ab>Grate <m><pa>brazilwood</pa></m> very finely, put it to soak one or two <ms><tmp>hours</tmp></ms> in <m>clear water</m>, then take this <m>tinted water</m> &amp; add to it some <m>clear water</m> &amp; you will make <del><fr>e</fr></del> <m>wine</m> as clear as you like. If you please, put a <ms>drop</ms> of <m>lemon or orange juice</m> in it &amp; it will immediately turn white. It can be drunk without danger.

</ab>

</div>

<div>

<id>p043v\_2</id>

<head><m>Pearls</m></head>

<ab>It is said that <m>pulverised talc</m> blown into a <tl>lamp</tl> renders them thus.

</ab>

</div>

<div>

<id>p043v\_3</id>

<head><pro>Arquebusier</pro></head>

<ab>To shoot your arquebus precisely the end of the breech must come precisely on the edge of the light, because like this the <m>powder</m> catches <x>fire</x> and burns all at once without blowing and has more strength and does not recoil. On the contrary, if the breech is made hollow, as they commonly are, the <m>powder</m> catches more quickly in this place, makes it recoil, and blows. This is clearly shown <x>by</x> a arquebus with a chamber which recoils more than another. And since the cannon is bigger at the breech than at the muzzle the sights are also uneven, because that at the breech is higher than that at the muzzle. Additionally, the thickness of the cannon is greater than the caliber by about one line, and the sight by another. It would therefore be necessary to either make the cannon all of one size or to raise the barrel from the end and towards the muzzle, and push it in and lower towards the breech. The weight of the <m>powder</m> must be one third of the <x>weight of the</x> bullet.

</ab>

</div>

<div>

<id>p043v\_4</id>

<head>Hail shot for the arquebus</head>

<ab>If you want that it stays together put a piece of <m>felt</m> or <m>leather</m> or <m>paper</m> on it, depending on the distance, and let the piece be made with a form precisely cut depending on the caliber of the arquebus.

</ab>

</div>