<page>044v</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f94.image</image>

<div>

<id>p044v\_1</id>

<head><m><al>Horse</al>hair sieves</m></head>

<ab>They are made often in <pl>Normandy</pl> with <m><al>horse</al>tail hairy</m> that they clean with some washing <m>water</m> because they pick them out with their mouth and separate short and broken ones. They do not make the <m>thread</m> longer than the sieve and it is round. They attach the black or white <m>hair</m> at the two edges of the thread, according to the piece they want to make. And the thread is woven above and below like any other fabric. And passing a small flat stick of ii or three fingers wide between two, they pass between after two bits of hair at each step strike and weave with three steps. The entire sieve is made of xvii bits of <m>hair</m>. They sell them by dozens and each xxx sols. They bring them to <pl>Toulouse</pl> to send them then to <pl>Spain</pl> and there, they exchange it with <m>silk</m>.</ab></div>

<div>

<id>p044v\_2</id>

<head>Excellent <m>water</m> against the pest by the Master of Montorsin</head>

<ab>Take some <m>theriac rue</m>, dittany and good <m>vinegar</m>, put the whole in a <m>glass</m> bottle and leave it half-open and well attached. And put it in a bath for three or 4 days. Then take some of your brew from its container when you need it and pour some, when necessary, on a red hot tile and receive the vapor and also perfume your clothes. This is a very precious and proved secret.</ab></div>

<div>

<id>p044v\_3</id>

<head><m>White soporific oil</m></head>

<ab>Have x or 12 <m>Mandragore apples</m>, put them in quarters together with some <m>olive oil</m> in a glass bottle which you will cook in a bain marie for two days and your <m>oil</m> will turn white with which you rub the sole of your feet and you will quickly feel sleepy.</ab></div>

<div>

<id>p044v\_4</id>

<head><m>Stucco</m></head>

<ab>For <m>glueing</m> <m>stone</m>, some do not use <del><fr>poi</fr></del> <m>resin</m> &amp; <m>black pitch resin</m> because it is too fatty, but take <m>rosin</m> &amp; <m>sulphur</m>, <ms>as much <del>as</del> of one as the other</ms>, &amp; as much of

<m>wax</m> as the two, and mix it with <m>crushed brick</m> for greater strength. Others, <m>white chalk</m> or <m>crushed &amp; pulverized &amp; sieved white stone</m>.</ab></div>