<page>045v</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f96.image</image>

<div>

<id>p045v\_1</id>

<head>Loading an arquebus</head>

<ab>You ought to have different charges according to the range that you want to give to your arquebus, all of which should have a screw on the end that fits in the nut of the the ramrod of the said arquebus. Thus, when you have put the powder in the charge, which is in the nut, hold the ramrod upright. And raising your arquebus up, insert the said ramrod until the charge is at the bottom of the arquebus, then right the arquebus, the mouth of the barrel up, and remove the ramrod. Thus your powder will be entirely in the breech without any of its grain or dust attaching to the sides of the arquebus, which always has some filth in the chamber. Thus it will not push back, and you will shoot more true.</ab>

<figure>

<id>fig\_p045v\_1</id>

<link>https://drive.google.com/open?id=0B9-oNrvWdlO5ZlVWTkcyU2FfanM</link>

</figure>

</div>

<div>

<id>p045v\_2</id>

<head>For adjusting an untrue cannon</head>

<ab>Take off the breech and place it on an even &amp; well-leveled table and pass through the inside a very even string without knots, on each end of which there should be a plumb hanging from each side. Then look into the barrel along the string, and if it does not touch equally all over, note the place where it does not touch &amp; hit with a hammer on the outside on that side &amp; in the same place, &amp; thus it will be righted, &amp; do thus all the way round.</ab>

</div>