<page>070v</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f146.image</image>

<div>

<cont/>

<id>p069r\_2</id>

<ab><m>Copper</m> <del>is bett</del> and <m>latten</m> are proper to cast &amp; at the right heat when they cast, while stirring them in the <tl>crucible</tl>, a very white flame &amp; that the bath is very liquid.</ab>

<ab>Some cast in <m>well ground <fr>ceruse</fr></m>, <del><fr>pour le</fr></del>; others in <m>flour</m> moistened several times with <m>oil</m> <del>&amp; <fr>g</fr></del> &amp; dried <env>in the sun</env>.</ab>

<ab>Others, for casting in <m>lead</m>, <m>old letters of <pro>printers</pro></m> or <m>types for the setting of letters</m>.</ab>

<ab>Others put into the <m>tin</m> or <m>lead</m> a substance of <m>fixed quicksilver</m> which makes it run.</ab>

</div>