<page>078v</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f162.item</image>

<div>

<id>p078v\_1</id>

<head>For making <m>bronze</m> in steel color</head>

<ab>Take <m><fr>alun de glace</fr></m> &amp; <m>antimony</m>, but one needs <ms>twice as much</ms> <m><fr>alun de glace</fr></m> as <m>antimony</m>, and pound it together into an <tl><m>iron</m> mortar</tl>, &amp; then mix with <m>gum water</m> while grinding it on <tl><m>marble</m></tl>, &amp; then one needs to use it with a <tl><fr>pinceau</fr></tl>, &amp; next let it dry, and then polish it with one <tl>tooth of a <al>wolf</al> or <al>dog</al></tl>.</ab>

</div>

<div>

<id>p078v\_2</id>

<head>For making <m>bronze</m> in gold color</head>

<ab>Take <m>copper filings</m> &amp;<m>ochre</m> &amp; <m>gum</m> &amp; <m>alum</m>, &amp; grind it all together into a <tl><m>stone</m> mortar</tl>, and when it is well ground, you will lay it on the work with a <tl><fr>pinceau</fr></tl>, then polish it with one <tl>tooth of a <al>wolf</al> or <al>dog</al></tl>.</ab>

</div>

<div>

<id>p078v\_3</id>

<head>For making <m>bone</m> or <m>horn</m> green</head>

<ab>Take <m>verdigris</m> &amp; mix it with <m>strong vinegar</m>, then soak your <m>bone</m> or <m>horn</m> one <ms><tmp>hour</tmp></ms>, &amp; then put on work.</ab>

</div>

<div>

<id>p078v\_4</id>

<head>For making <m>bronze</m></head>

<ab>Take <m>filings of pin</m> &amp; other of <m>latten</m>, &amp; put it together, &amp; grind it on <tl><m>marble</m></tl>, grind it well with <m>water</m> little by little, until it is distilled, then put them into some new <tl>vessel</tl>. And</ab>

<cont/>

</div>