<page>102r</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f209.image</image>

<div>

<id>p102r\_1</id>

<head>Provisions for the work of Colchis</head>

<ab>7 <tl>retorts</tl>

2 <ms>lb.</ms> of <figure><del><m>☿</m></del></figure> <figure><m>☿</m></figure>

One measure of <m>coarse salt</m>

6 <tl><fr>terrines</fr> without <m>lead</m></tl>

2 large <tl><m>unleaded</m> pots</tl> for calcining

2 <tl>alembics</tl> for distilling <m>vinegar</m>

4 <tl><ms>pots</ms></tl> of <m>good vinegar</m>

3 or 4 <tl>lamps</tl>

2 <ms>lb.</ms> of <m>cotton</m>

One pair of small <tl>scissors</tl></ab>

</div>

<div>

<id>p102r\_2</id>

<head>For the <tl>furnace</tl></head>

<ab>A <tl>coffer</tl> with a <m>stone</m> ten <ms>square <bp><fr>thumbs</fr></bp></ms> in size, and one <ms><bp><fr>foot</fr></bp></ms> thick, pierced in the middle

2 <m>earthenware</m> <tl>boxes</tl> or <tl> pots with a lid</tl>

2 small <tl>pipes of <m><fr>fer blanc</fr></m></tl> to evacuate the smoke from the <tl>furnace</tl>

<m><pa>Rapeseed</pa> oil</m> for the <tl>lamps</tl> to heat the <tl>furnace</tl>

A <tl>fire-steel</tl></ab>

</div>

<div>

<id>p102r\_3</id>

<head><m>Royal cement</m></head>

<ab>One <ms>lb. &amp; a half</ms> of <m>vitriol</m>

As much <m>saltpeter</m>

As much <m>rock alum</m></ab>

</div>

<div>

<id>p102r\_4</id>

<head><tl><m>Glass</m> vessels</tl></head>

<ab>The <tl><m>glass</m> vessel</tl> must be made like a pear or round pyramid, of the thickness as a <ms>small <tl>knife</tl> back</ms>, round on the bottom without bending like <tl>vials</tl>, its opening of such a size that a <tl><ms><pl>Dutch</pl> quill</ms></tl> can just about fit in, &amp; with a lip at the end. Thus of height of seven <ms><bp>fingers</bp>' width</ms>.

<figure>

<id>fig\_p102r\_1</id>

<margin>bottom</margin>

<link><https://drive.google.com/open?id=0B9-oNrvWdlO5MVhNYTRzOXJzR2M></link>

</figure>

</ab>

</div>