<page>005v</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f16.image</image>

<div>

<cont/>

<id>p005r\_a2</id>

<ab>string &amp; will reflect a <bp>nipple</bp> as large as a plate, and women can see the secret places that they do not want to show to <pro>surgeons</pro>. It casts the representation out of itself, and if you touch with your <bp>finger</bp> the eye of the representation, another <bp>finger</bp> will come against yours.</ab>

<ab>You will be able to make a light at night for someone quite far away, if you place the concave mirror behind a candle placed on the window sill. You can read and write quite far from the candle if you place it behind the candle &amp; place &amp; turn the concavity towards you. If you put the mirror at the end of a table &amp; a candle on it, it will represent two lights on the table for you. To see what is happening on a street, shutter the window, or the more you can shut the better, make a hole in the bottom <sup>pane</sup>, the size of your <ms><bp>little finger</bp></ms>, perfectly round all the way through. Then apply a sheet of paper onto the window and let the middle of the sheet be over the hole. Pierce the sheet in the same place as the hole and of the same size. Then turn the concave face of the mirror towards the hole, and anyone passing by in the street will be reflected on the sheet of paper. Do the same with the pierced door of a closed room. You can make wavy <sup>mirrors</sup> and triangular ones, such as are described by Ptolemy and Archimedes. The concave sort can also set fire to straw or light a candle from afar, using the sun. By reverberating fire too, it can provide warmth.</ab>

</div>  
<div>  
<id>p005v\_a1</id>  
<head>For bronzing in yellow and white</head>

<ab>Take <m>mirror tin</m> and melt it. On half a pound of this, put half an ounce of <m>quicksilver</m>, and remove it immediately from the fire and grind it until it is like ashes. Wash it thoroughly in <m>clean water</m>, then grind it on a <tl><m>marble</m> slab</tl> and soak it with water of <m>glue de retailles</m>. Then apply that on your wooden candlesticks and any other works you like, and burnish with a <m>tooth</m>. You can grind <m>pin filings</m> and apply them with the said <m>glue <sup>de retailles</sup></m>. </ab>

</div>