<page>045r</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f95.image</image>

<div>

<id>p045r\_1</id>

<head>Loading an arquebus with a <m>hail shot</m> </head>

<figure>

<id>fig\_p045r\_1</id>

<link><https://drive.google.com/open?id=0B9-oNrvWdlO5bkhmQklfNHJoRnc></link>

</figure>

<ab>One needs to make a <m>wooden</m> pipe as long as the width of 4 or 5 fingers, which should be hollowed precisely according to the mouth of your barrel, of the form represented in <del>D</del> A. Then, having cut strong <m>paper</m>, <del>of the</del> as of large printed books, in the form of D, as wide as you want to make your cartridge<comment>c\_045r\_01</comment> long, wrap the <m>paper</m> around the baton B &amp; at the end, where the point F will be, fold it all around the said <m>paper</m>, &amp; your cartridge will be formed. But, in order to make the bottom more uniform, put it into pipe A, then put in the baton B and, through the other end of the pipe, which is marked G, put the baton C &amp;beat so as to tamp &amp; press the folded tip of your cartridge, then take it out, &amp; load it. Put three or four <fr>drageons</fr><comment>c\_045r\_02</comment> or tears<comment>c\_045r\_03</comment> into it. Then, with a cutting-punch, marked E, which should be of the same caliber as your arquebus or pistol, punch round pieces on <m>cardboard</m> or <m>felt</m> or <m>waxed cloth</m>, and put this round piece into your cartridge, and push it onto the <fr>drageons</fr> with the baton B. Next, more <fr>drageons</fr>, 3 or 4, then a round piece. And do thus until the cartridge is full, then put it into your arquebus. If you want your hail shot to scatter sooner, make the round pieces out of <m>paper</m>. If you want it to reach farther without scattering, make the piece out of <m>cardboard</m>. If you want even farther, make the round piece out of <m>waxed cloth</m>, or else of <m>leather</m> or <m>felt</m>, &amp; a piece of <m>waxed cloth</m> on the top. And if you make the cartridge itself of <m>waxed cloth</m> or <m>waxed paper</m>, it will reach one hundred paces &amp; will make for great piercing, &amp; the hail shot, barely scattering, will make an opening. But if you make your cartridge with <m>waxed cloth</m> or a material stronger than <m>paper</m>, you ought not to make it so long from the square coming to the point as in D, because it is enough that it makes two turns. <figure>#</figure>In this manner, the <m>hail shot</m> barely scatters &amp; makes for great piercing against a door, body of a cuirass<comment>c\_045r\_04</comment>, and others.</ab>

<ab>

<margin>left-middle</margin>

<x><figure>#</figure></x> as <del>D</del> H

</ab>

</div>