<page>073r</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f151.image</image>

<div>

<id>p073r\_1</id>

<head>For making <m>blue varnish</m></head>

<ab>Take the <m>blue of flowers <add>florey or of <pl>Flanders</pl></add></m> &amp; <m>quicklime</m>, and put in around four <ms><bp>fingers</bp></ms> of <m>water</m>, and let it soak one <ms><tmp>day</tmp></ms>. Take the <m>water</m> where the said <m>quicklime</m> has soaked, and put your <m>blue</m> with it, and lay it down <corr>on</corr> the <m>wood</m>.</ab>

</div>

<div>

<id>p073r\_2</id>

<head>For orange color</head>

<ab>Take <m>water</m> where the <m>quicklime</m> has soaked and put <m><fr>terroy merita</fr></m>, and put them one with the other, and then set on your <m>wood</m>.</ab>

</div>

<div>

<id>p073r\_3</id>

<head>For ridding <m>bone</m> or <m>horn</m> of fattiness</head>

<ab>One needs to make them boil in <m>quicklime</m>, and it must always have <m>water</m>, and take a very clean <tl>pan</tl>. And when they are washed, make them boil in the <m>ashes of <pa>vine shoots</pa></m>, and put them inside the hottest <tl>pot</tl> you can, and put <m>verdigris</m> into the <tl><m><pro>goldsmith's</pro> water</m> pot</tl>, and leave for the space of some time, and you will see a very beautiful green color.</ab>

</div>

<div>

<id>p073r\_4</id>

<head>For making gray <m>wood</m></head>

<ab>Take <m>alum</m> with <m>river water</m>, make them boil together, then take <m>river water</m> with <m>bran</m>, submerge the <m>bran</m> and beat it together. Take <m>iron filings</m> &amp; <m>sulfur</m> &amp; <m>verdigris</m> and <add><m>fuller's earth</m></add> <gap/>, and make it all boil together, and pound <m><pa>maplewood</pa></m> which will have been soaked in <m>water of alum</m> and <m>well water</m>, &amp; put it to boil together. <add>All of this will be done better in hollow <m>sandstone</m>.</add></ab>

</div>

<div>

<id>p073r\_5</id>

<head>For making <m>bronze</m> in gold color</head>

<ab>Take one <ms>ounce</ms> of <m>sal ammoniac</m> and grind it in an <tl><m>iron</m> mortar</tl>. Once well ground, take one <ms>ounce</ms> of <m>sulfur</m>, and

</ab>

<cont/>

</div>