<page>076v</page>

<image>http://gallica.bnf.fr/ark:/12148/btv1b10500001g/f158.item</image>

<div>

<id>p076v\_1</id>

<head>For making very beautiful gold color &amp; of little expense</head>

<ab>First take very yellow <m><pa>orange</pa> peel,</m> &amp; clean them well of the white that is inside, &amp; pulverize them very well <del>and</del> <add>in</add> a very clean <tl>mortar</tl>. And take as much of <m>sulphur</m>, &amp; grind all together, and put everything in a <tl><m>glass</m> vial</tl>, &amp; keep them <env>in the cellar or other damp place</env> for the space of eight or ten <ms><tmp>days</tmp></ms>. Then when you want to use it, one needs to warm it and use it where you want, &amp; you will see a very beautiful color. </ab>

</div>

<div>

<id>p076v\_2</id>

<head>For making black <m><fr>goumiche</fr></m></head>

<ab>

Take some <m>glue</m>, &amp; mix it with <m>vinegar</m>, &amp; melt it until and it should be very clear. And take <m>lampblack</m> or another black &amp; mix them together, then lay it on <m>wood</m>.</ab>

</div>

<div>

<id>p076v\_3</id>

<head>For the white </head>

<ab>One needs to take <m>white wax</m> with <m>ceruse</m>, and melt all together, &amp; lay it on <m>wood</m> or another thing.</ab>

</div>

<div>

<id>p076v\_4</id>

<head>For gilding <m>iron</m> or <m>tin</m></head>

<ab>First one needs to wash that which one wants to gild in <m>wine lees</m>, and then wash it again with <m>white wine</m>, and take three <ms>ounces</ms> <m><fr>terra merita</fr></m> &amp; a <ms>chopin</ms> of <m>white wine</m>, and boil the substances the <ms>space of <tmp>half an hour</tmp></ms>, &amp; apply your colors on your <m>iron</m> or <m>tin</m>, or other, and then let it dry on a piece of <tl><m>paper</m></tl>, &amp; not put the <bp>hand</bp> in your substances.</ab>

</div>